Optimized Single Speed:

|  |  |  |  |
| --- | --- | --- | --- |
| **Motor** | **Avg Velocity (mph)** | **Energy Req (kWh)** | **Front/Rear Sprocket** |
| Emrax 268 | 124.97 | 20.0097 | 21/29 |
| Remy HVH 250 90s | 136.783 | 29.4321 | 21/50 |